# Address "0x0"; Register "REG1"

Register: reg desc

Address : 0x0

Reset Value : 0x603

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Field Name | Bits | Access Type | Reset Value | Description |
| field1 | [ 3: 0] | RW | 0x3 | field desc |
| field2 | [ 8: 4] | RO | 0x0 | field desc |
| field3 | [10: 9] | RO | 0x3 | field desc |
| reserved | [31:11] | RO | 0x0 | field desc |

# Address "0x4"; Register "REG2"

Register: reg desc

Address : 0x4

Reset Value : 0x63

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Field Name | Bits | Access Type | Reset Value | Description |
| field1 | [ 3: 0] | RW | 0x3 | field desc |
| field2 | [ 4 ] | RO | 0x0 | field desc |
| field3 | [10: 5] | RW | 0x3 | field desc |
| field4 | [11 ] | RW | 0xA | field desc |